BMS 2. BMS - Beam Momentum Station - 256 ch of Hodoscopes Respondibble - Jen Bisplinghoff, Rainer Jahn 4 station of hodoscope - Location 135--60 m upsteam of polarized target 1 mm fingers, Step overlap 30% Photomultiplier XP...., lectronics- PM-Discrim - long cabel (310m )- Discrim. - Logic 4. HV - 8 pc HV power supply LeCroy 14032. Very old - 20 years. Very often had broken. Control by CAMAC interface. ( no scheme)

Discriminators in Barrak need to be change - may be will be like for Sci Fi Hodoscopes