ECAL1

2. ECAL 1 : Lead Glass calorimeter , 3300 ch Lead Glass 38x38 mm(GAMS 320 ch Lead Glass 140x140 mm.(OLGA) Responsible: S. Donskov. V. Polykov

3. Crate control VME 9U ---- min 4 crates with ADC system ; CANbus interface to PC CAMAC crate--- 1 pc for LED driver, for Small Motors driver, for Big Motors Driver NIM crate ------ 1-2 pc

4. HV; Power supply - 4 pc Heinzinger f or 3300ch. .. Range of HV = 2000V

Boosters power supply: ---- 8 pc. Type ---- Oltronics . V. Range--- 200 -500V.

HV power supply for 320 ch Big Lead Glass -- tbd

Monitoring of V, ON/OFF, MAINS (220) 5. LV 6. Analog monitoring Temperatura inside the Cassete -------- 4 pc T sensor Smoke sensor-------------------------2pc 7.Boolen Position sensor -------------5 pc(Top, Bottom, Left, Right, Central) 8.Start -up . Manually 9 Special pr ocedur es. . Setting HV for every channel. .. Calibration of each cell by mo ving cassete though e- beam. in X/Y dir ection.. C

. Pedestal monitoring Comparison of new table with pedestal with pr evious one deviation +/- N counts - Normal ; if value of one or some is equal = 0 --- Warning ALARM if values of group channell = 0 Fatal ALARM

4. Gain monitoring Monitoring of Gain by LED(Laser) monitoring systemComparison of new table with LED signals with pr evious one deviation +/- N counts - Normal ; if value of one or some is equal = 0 --- Warning ALARM if values of group channell = 0 Fatal ALARM 11 Trending Pedestal stability Gain stability .