HCAL2

2. HCAL2 ; Hadr on calorimeter , 220 cells, Sandvich : Steel -20 mm; Scitilator -5 mm Dim. - 3 x 4 meters Respondsible - Polykov.V 3. Crate contr ol VME 9U - crate for ADC, readout by DAQ CAMAC crate for electronics of LED driver, Bases motors Driver NIM crate Monitoring : V, I , T 4. HV Power Supply - Heinzinger 2500 -0,4------- 1 pc Monitoring outputs for V and I Boosters Power supply - 200-500V Oltronics --4 pc

5. LV Power Supply - +/- 6V for preAmplifiers .----- ? 6.Analog monit

7. Boolen. End Position points , Central point-------------- 3 pc 8. Start-up Operator manuall 9. Special pr ocedur e 1. Pedestal monitoring Special Monitoring task sinchronise with START BEAM send artificial signal GATE for ADC system and read data from DAQ. The table with average values of pedestals is load to ADC pedestal memories and compare with previous one deviation +/- N counts - Normal ; if value of one or some is equal = 0 --- Warning ALARM if values of group channell = 0 Fatal ALARM

2. Gain monitoring Special monitoring task synchronise to the END of SPILL trigger Light source and read data from DAQ. The table of values of LED signals compare with previou one. deviation +/- N counts - Normal ; if value of one or some is equal = 0 --- Warning ALARM if values of group channell = 0 Fatal ALARM

11. Trernding Pedestal stability---table of Pied Gain stability -- table of LED

12. Data saving to DAQ Piedestals table, LED signal table