COMPASS RICH 1

.

• radiator : C_4F_{10} , length: ∼ 3 m

• mirrors :

spherical, focal length: 3.3 m, reflectance > 80% for λ > 165 nm, total surface: (5.3 * 4) m^2

• photon detectors: MWPC’s with CsI photocathodes, out of spectrometer acceptance, total active surface: 5.3 m^2

• read-out electronics :

analog read-out (mainly for good efficiency), 83 K channels in total, av. expected occupancy: ∼ 5 % , total maximum data flux: 2.5 GB / sec in spill