STATUS OF COMPASS RICH-1, May 23, 2000

• vessel (80 m^3): delivered,

weldings checked: no leakages

• vessel windows (2 light composite panels,

total surface: ∼ 25 m^2): delivered, ready to be mounted

• mirror wall mechanics (∼ 20 m^2): completely assembled

• radiator gas system (C_4F_{10}):

ready, commissioned

• photon detectors (MWPCs with CsI photocathodes):

4 (over 8) detectors assembled, ready to be mounted onto the vessel

• mirrors: 10 pieces (over 120) ready and mounted, alignment (angular regulation) during these days