TRIGGER

2. TRIGGER HODOSCOPEs, HARDRON CAL. TRIGGER

Urgen Hannapelle, Sandro Bravar 500 ch hodoscopes -- 2000 800 ch hodo.----------2001 Short dicriptions : Scintil. hodoscopes - Dscriminators -- Logic(computer control) Trigger for Hcal : Adders, 4-1, --- 16- 1 -- Discrim -- Logic SUM. 3. Crates NIM - 2pc VME -------1-2pc for Logic and Discrim VME 9-------2-3 pc Readout Homemade Crates - 2 pc for HCAL Trigger Monitoring of Crate ------all parameters 4. HV.

500 ch ----next year 1000ch -----2001 y CAEN -----?

LeCroy------? depends of money Now -------LeCroy4032 , if like now - 30pc of HV crates Monitoring -- V, I, ON/OFF, Ramp up/ Ramp down Speed of monitoring --- as DCS is posible 5 .LV +/- 5V, --- 50 pc. in barrak or outside

6.Analog monitoriing Temperatura - inside of hodoscopes --------10-20ch 60 sec Humidity in crates Magnetic field --------------- Position ---------------------TV camera 7.Start up Manualy LOad latest Running version 8 Special procedure Loading Thresholds - 1000ch through VME Loading Delay table 9. Boolen--------------------NO 10.ALARMS 11. Trending with 01.% dead-band for 1 week 14Requirements of SD TV monitoring of position, motorized PC with Linux P